Title: Re: [luau] Networking Question
Last saved by: Ben Beeson

Titel: Re: [luau] Networking Question | 7/8/01
URL: /tmp/soffice.tmp/sv8466.tmp/mail8566.htm | 14:00:29

Marcus,

	I am replying to you and the list here, I apologize for not keeping all this on the list. Anyway, the cable has been specifically built and tested for directly connecting two computers.  It worked great recently, then I had a hardware failure (new motherboard and fresh install of a new OS as a result) As I rebuild, I'm changing a few things around so a simple restore won't work here...

Thanks again,

Ben 

>>>>>>>>>>>>>>>>>> Original Message <<<<<<<<<<<<<<<<<<

On 7/7/01, 8:46:06 PM, "Marcus Patino" <manou69@hotmail.com> wrote regarding Re: [luau] Networking Question:

> OK now - I just read the email dusty put out on the list and realized that
> it may have your answer.  If you do have a rollover cable then some of the
> pairs may not be right - check this site
> http://www.siriuscomputers.com/rj45.htm.  it shows the 2 cable styles that
> most networks should use - to my knowledge - if you make one end the 'a'
> standard and the other the 'b' standard then you should be ok.  If the cable
> is just reversed then someof the wires may not be right but I am still
> working on that drawing myself - I know I asked before - but can you see the
> colors on the ends of the cables??

> M

> >From: Ben Beeson <beesond001@hawaii.rr.com>
> >To: Marcus Patino <manou69@hotmail.com>
> >Subject: Re: [luau] Networking Question
> >Date: Sun, 08 Jul 2001 02:45:33 GMT
> >
> >Marcus,
> >
> >     All the little green lights are on for the VALinux box.  The Sparc20
> >doesn't have any green lights, but if I run /sbin/ifconfig on both boxes,
> >it says that the interfaces are up and running. I can ping myself by IP
> >address and name on both machines, just not the other machine. Sample
> >output follows...
> >
> >Note the Valinux box has 2 NICs, so I checked both of them...
> >
> >[ben@a24b94n83client89 ben]$ ping localhost
> >PING VALinux (127.0.0.1) from 127.0.0.1 : 56(84) bytes of data.
> >64 bytes from VALinux (127.0.0.1): icmp_seq=0 ttl=255 time=77 usec
> >64 bytes from VALinux (127.0.0.1): icmp_seq=1 ttl=255 time=46 usec
> >64 bytes from VALinux (127.0.0.1): icmp_seq=2 ttl=255 time=42 usec
> >
> >--- VALinux ping statistics ---
> >3 packets transmitted, 3 packets received, 0% packet loss
> >round-trip min/avg/max/mdev = 0.042/0.055/0.077/0.015 ms
> >
> >[ben@a24b94n83client89 ben]$ ping 192.168.1.10
> >PING 192.168.1.10 (192.168.1.10) from 192.168.1.10 : 56(84) bytes of
> >data.
> >64 bytes from 192.168.1.10: icmp_seq=0 ttl=255 time=81 usec
> >64 bytes from 192.168.1.10: icmp_seq=1 ttl=255 time=44 usec
> >64 bytes from 192.168.1.10: icmp_seq=2 ttl=255 time=44 usec
> >
> >--- 192.168.1.10 ping statistics ---
> >3 packets transmitted, 3 packets received, 0% packet loss
> >round-trip min/avg/max/mdev = 0.044/0.056/0.081/0.018 ms
> >[ben@a24b94n83client89 ben]$ ping VALinux
> >PING VALinux (127.0.0.1) from 127.0.0.1 : 56(84) bytes of data.
> >64 bytes from VALinux (127.0.0.1): icmp_seq=0 ttl=255 time=84 usec
> >64 bytes from VALinux (127.0.0.1): icmp_seq=1 ttl=255 time=211 usec
> >
> >--- VALinux ping statistics ---
> >2 packets transmitted, 2 packets received, 0% packet loss
> >round-trip min/avg/max/mdev = 0.084/0.147/0.211/0.064 ms
> >[ben@a24b94n83client89 ben]$
> >
> >
> >Output from the sparc 20 looks similar.
> >
> >     As far as net speeds go, the NICs in the VALinux box are autosensing
> >10/100s.  I think the sparc NIC is able to do both also, but even if it
> >can't, the VALinux NICs are working with a cable modem right now, so I
> >know they can support the 10MHz end of the speed spectrum.
> >
> >     As far as the cable goes, I don't have a way to really check it other
> >than to say that it worked OK last time I had it hooked up, and I watched
> >the technician test it when he built it for me.
> >
> >     Are there any particular routing entries that I need to check?
> >
> >
> >
> >Thanks, I'll keep looking...
> >
> >Ben
> >
> >
> > >>>>>>>>>>>>>>>>>> Original Message <<<<<<<<<<<<<<<<<<
> >
> >On 7/7/01, 3:53:07 PM, "Marcus Patino" <manou69@hotmail.com> wrote
> >regarding Re: [luau] Networking Question:
> >
> >
> > > from everything I read this should work - unless the cable has gone bad
> >due
> > > to a kink or just a bad end.  I am going with this thinking that you can
> > > ping 127.0.0.1 from both mahcines without issue and that all lights are
> >on
> > > and ready.  Unless there is a speed issue with the cards - but I would
> >think
> > > that if both support either 10 or 100 then you should be working without
> > > issue - just for kicks - can you see the color patern on the ether
> >cable?? -
> > > maybe there is something not right there
> >
> > > M
> >
> >
> > > >From: Ben Beeson <beesond001@hawaii.rr.com>
> > > >To: Marcus Patino <manou69@hotmail.com>
> > > >Subject: Re: [luau] Networking Question
> > > >Date: Sun, 08 Jul 2001 01:13:49 GMT
> > > >
> > > >Marcus, or is it Marc?
> > > >
> > > >     I am trying to directly connect two boxes with one rolled ethernet
> > > >cable.  I am using subnet masks of 255.255.255.0 on both boxes.  At one
> > > >time I had one Linux box and a windoze box working this way with the
> >same
> > > >cable, but when I had a hardware failure, I had to rebuild everything.
> > > >Now I'm trying to use the sparc box in the place of the windoze box,
> >but
> > > >I can't remember how I did it last time.  Even if I could remember
> >that,
> > > >too much has changed so I am really re-inventing here...  Anyway, I'm
> >not
> > > >a network guru, just trying to learn.  I thought I'd start with
> >something
> > > >apparently simple.
> > > >
> > > >Thanks for any clues you may provide me with,
> > > >
> > > >Ben
> > > >
> > > >
> > > >
> > > > >>>>>>>>>>>>>>>>>> Original Message <<<<<<<<<<<<<<<<<<
> > > >
> > > >On 7/7/01, 1:14:16 PM, "Marcus Patino" <manou69@hotmail.com> wrote
> > > >regarding Re: [luau] Networking Question:
> > > >
> > > >
> > > > > I am trying to visuallize your setup - so bare with me - you say
> >rolled
> > > > > ehternet and then wan - I Am guessing you are using a corss over
> >cable
> > > >to
> > > > > driectly connect 2 systems? -
> > > > > If so then the only thing I can think of (if all the interfaces are
> >up
> > > >and
> > > > > configured) is that either the subnet masks are wrong or your cable
> >is
> > > > > messed up somehow - my icq is 4777985 - I would like to know more of
> > > >what
> > > >is
> > > > > going on here  - fell free to message me or just reply back to this
> > > >email
> > > >
> > > > > M
> > > >
> > > >
> > > > > >From: Ben Beeson <beesond001@hawaii.rr.com>
> > > > > >Reply-To: "Linux & Unix Advocates & Users" <luau@list.luau.hi.net>
> > > > > >To: "Linux & Unix Advocates & Users" <luau@list.luau.hi.net>
> > > > > >Subject: [luau] Networking Question
> > > > > >Date: Sat, 07 Jul 2001 22:45:26 GMT
> > > > > >
> > > > > >Aloha all,
> > > > > >     I am still trying to get my two computers to talk to each
> >other at
> > > >home.
> > > > > >  Here is a brief rundown on what I have to work with and what I
> >want
> > > >to
> > > > > >do.  I have one VALinux StartX MP and a Sparc20.   Both machines
> >are
> > > > > >running RedHat Linux 6.2, one version for Intel, one for Sparc.  I
> >am
> > > > > >using a rolled ethernet cable to connect the two boxes. My VALinux
> >box
> > > > > >will use the IP address 192.168.1.10 and is named "VALinux."  The
> > > >Sparc20
> > > > > >is 192.168.1.20 and is called "sparky."  So far the name and IP
> > > >addresses
> > > > > >lookup OK, but I cannot ping, ssh, or telnet across the LAN yet.
> >Any
> > > > > >ideas what I should try next, or where I should look to fix this??
> > > > > >Thanks in advance,
> > > > > >Ben
> > > > > >
> > > > > >
> > > > > >
> > > > > >---
> > > > > >You are currently subscribed to luau as: manou69@hotmail.com
> > > > > >To unsubscribe send a blank email to
> >leave-luau-472M@list.luau.hi.net
> > > >
> > > > > _________________________________________________________________
> > > > > Get your FREE download of MSN Explorer at http://explorer.msn.com
> >
> > > _________________________________________________________________
> > > Get your FREE download of MSN Explorer at http://explorer.msn.com

> _________________________________________________________________
> Get your FREE download of MSN Explorer at http://explorer.msn.com

Page  from 1